The included file uses the MicroBlaze to control a custom peripheral that provides video loopback & colorbars.

Intended use is the Avnet A/V module plugged into the P2 connector of the Avnet Virtex II Development Board.
This file has also been included in the SystemACE MPM file.  See the MPM directory.



To control the test, set your VT100 compatible terminal as follows:
19200, 8, N, 1, No flow control

Use DIP Switch 1 for Reset.

At the terminal interface ("ADS>" prompt) enter "help" for a list of commands.
