The av_test.mpm file is generated for the A/V module plugged into the P2 connector of the Avnet Virtex II Development Board.  This file may be programmed into the SystemACE device on the Virtex II Development Board and tests individually selected as follows:

	JP103 = 000 = Audio CODEC loopback test
	JP103 = 001 = VGA Monitor Color Bars
	JP103 = 010 = Video capture to TV encode

The selected test will be run at power up or reset (SW1).