The AC97_xxx.vhd will place the audio CODEC in loopback mode (Line in to Line out) via the CODEC's AC97 interface.  The AC97_top_0424_gold.bit file is generated for the A/V module plugged into the P2 connector of the Avnet Virtex II Development Board.